


Router0:















Router1:















Router2:















Router3:













Connectivity:




IP Routes:


Router0:




Router1:



Router2:




Router3:




Metrics:


Router0:




Router1:



Router2:



Router3:



Comparison:

Default metric = [10^7/K1\*Min bandwidth + K3\*Total Sum of delay(usec)/10] \* 256

=[10^7/1\*128+1\*20000/10]\*256

=229890560